{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["劳务报价单"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"劳务报价单","index":0,"n_rows":254,"n_cols":10,"rows_kept":254,"merged":[[0,0,0,9],[1,0,1,3],[1,4,1,6],[1,7,1,9],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,4],[2,5,3,5],[2,6,3,7],[2,8,2,9],[4,3,4,4],[4,6,4,7],[5,3,5,4],[5,6,5,7],[6,3,6,4],[6,6,6,7],[7,3,7,4],[7,6,7,7],[8,3,8,4],[8,6,8,7],[9,3,9,4],[9,6,9,7],[10,3,10,4],[10,6,10,7],[11,3,11,4],[11,6,11,7],[12,3,12,4],[12,6,12,7],[13,0,13,8],[14,0,14,9],[15,0,15,3],[15,4,15,6],[15,7,15,9],[16,0,17,0],[16,1,17,1],[16,2,17,2],[16,3,17,4],[16,5,17,5],[16,6,17,7],[16,8,16,9],[18,3,18,4],[18,6,18,7],[19,3,19,4],[19,6,19,7],[20,3,20,4],[20,6,20,7],[21,3,21,4],[21,6,21,7],[22,3,22,4],[22,6,22,7],[23,0,23,8],[24,0,24,9],[25,0,25,3],[25,4,25,6],[25,7,25,9],[26,0,27,0],[26,1,27,1],[26,2,27,2],[26,3,27,4],[26,5,27,5],[26,6,27,7],[26,8,26,9],[28,3,28,4],[28,6,28,7],[29,3,29,4],[29,6,29,7],[30,3,30,4],[30,6,30,7],[31,3,31,4],[31,6,31,7],[32,3,32,4],[32,6,32,7],[33,3,33,4],[33,6,33,7],[34,3,34,4],[34,6,34,7],[35,3,35,4],[35,6,35,7],[36,3,36,4],[36,6,36,7],[37,0,37,8],[38,0,38,9],[39,0,39,3],[39,4,39,6],[39,7,39,9],[40,0,41,0],[40,1,41,1],[40,2,41,2],[40,3,41,4],[40,5,41,5],[40,6,41,7],[40,8,40,9],[42,3,42,4],[42,6,42,7],[43,3,43,4],[43,6,43,7],[44,3,44,4],[44,6,44,7],[45,3,45,4],[45,6,45,7],[46,3,46,4],[46,6,46,7],[47,3,47,4],[47,6,47,7],[48,3,48,4],[48,6,48,7],[49,0,49,8],[50,0,50,9],[51,0,51,3],[51,4,51,6],[51,7,51,9],[52,0,53,0],[52,1,53,1],[52,2,53,2],[52,3,53,4],[52,5,53,5],[52,6,53,7],[52,8,52,9],[54,3,54,4],[54,6,54,7],[55,3,55,4],[55,6,55,7],[56,3,56,4],[56,6,56,7],[57,3,57,4],[57,6,57,7],[58,3,58,4],[58,6,58,7],[59,0,59,8],[60,0,60,9],[61,0,61,3],[61,4,61,6],[61,7,61,9],[62,0,63,0],[62,1,63,1],[62,2,63,2],[62,3,63,4],[62,5,63,5],[62,6,63,7],[62,8,62,9],[64,3,64,4],[64,6,64,7],[65,3,65,4],[65,6,65,7],[66,3,66,4],[66,6,66,7],[67,3,67,4],[67,6,67,7],[68,0,68,8],[69,0,69,9],[70,0,70,3],[70,4,70,6],[70,7,70,9],[71,0,72,0],[71,1,72,1],[71,2,72,2],[71,3,72,4],[71,5,72,5],[71,6,72,7],[71,8,71,9],[73,3,73,4],[73,6,73,7],[74,3,74,4],[74,6,74,7],[75,3,75,4],[75,6,75,7],[76,3,76,4],[76,6,76,7],[77,3,77,4],[77,6,77,7],[78,3,78,4],[78,6,78,7],[79,3,79,4],[79,6,79,7],[80,0,80,8],[81,0,81,9],[82,0,82,3],[82,4,82,6],[82,7,82,9],[83,0,84,0],[83,1,84,1],[83,2,84,2],[83,3,84,4],[83,5,84,5],[83,6,84,7],[83,8,83,9],[85,3,85,4],[85,6,85,7],[86,3,86,4],[86,6,86,7],[87,3,87,4],[87,6,87,7],[88,3,88,4],[88,6,88,7],[89,3,89,4],[89,6,89,7],[90,3,90,4],[90,6,90,7],[91,3,91,4],[91,6,91,7],[92,3,92,4],[92,6,92,7],[93,3,93,4],[93,6,93,7],[94,0,94,8],[95,0,95,9],[96,0,96,3],[96,4,96,6],[96,7,96,9],[97,0,98,0],[97,1,98,1],[97,2,98,2],[97,3,98,4],[97,5,98,5],[97,6,98,7],[97,8,97,9],[99,3,99,4],[99,6,99,7],[100,3,100,4],[100,6,100,7],[101,3,101,4],[101,6,101,7],[102,3,102,4],[102,6,102,7],[103,3,103,4],[103,6,103,7],[104,3,104,4],[104,6,104,7],[105,0,105,8],[106,0,106,9],[107,0,107,3],[107,4,107,6],[107,7,107,9],[108,0,109,0],[108,1,109,1],[108,2,109,2],[108,3,109,4],[108,5,109,5],[108,6,109,7],[108,8,108,9],[110,3,110,4],[110,6,110,7],[111,3,111,4],[111,6,111,7],[112,3,112,4],[112,6,112,7],[113,3,113,4],[113,6,113,7],[114,3,114,4],[114,6,114,7],[115,3,115,4],[115,6,115,7],[116,3,116,4],[116,6,116,7],[117,3,117,4],[117,6,117,7],[118,3,118,4],[118,6,118,7],[119,0,119,8],[120,0,120,9],[121,0,121,3],[121,4,121,6],[121,7,121,9],[122,0,123,0],[122,1,123,1],[122,2,123,2],[122,3,123,4],[122,5,123,5],[122,6,123,7],[122,8,122,9],[124,3,124,4],[124,6,124,7],[125,3,125,4],[125,6,125,7],[126,3,126,4],[126,6,126,7],[127,3,127,4],[127,6,127,7],[128,3,128,4],[128,6,128,7],[129,0,129,8],[130,0,130,9],[131,0,131,3],[131,4,131,6],[131,7,131,9],[132,0,133,0],[132,1,133,1],[132,2,133,2],[132,3,133,4],[132,5,133,5],[132,6,133,7],[132,8,132,9],[134,3,134,4],[134,6,134,7],[135,3,135,4],[135,6,135,7],[136,3,136,4],[136,6,136,7],[137,3,137,4],[137,6,137,7],[138,3,138,4],[138,6,138,7],[139,3,139,4],[139,6,139,7],[140,3,140,4],[140,6,140,7],[141,3,141,4],[141,6,141,7],[142,3,142,4],[142,6,142,7],[143,3,143,4],[143,6,143,7],[144,3,144,4],[144,6,144,7],[145,3,145,4],[145,6,145,7],[146,3,146,4],[146,6,146,7],[147,3,147,4],[147,6,147,7],[148,3,148,4],[148,6,148,7],[149,3,149,4],[149,6,149,7],[150,3,150,4],[150,6,150,7],[151,3,151,4],[151,6,151,7],[152,3,152,4],[152,6,152,7],[153,3,153,4],[153,6,153,7],[154,3,154,4],[154,6,154,7],[155,3,155,4],[155,6,155,7],[156,3,156,4],[156,6,156,7],[157,0,157,8],[158,0,158,9],[159,0,159,3],[159,4,159,6],[159,7,159,9],[160,0,161,0],[160,1,161,1],[160,2,161,2],[160,3,161,4],[160,5,161,5],[160,6,161,7],[160,8,160,9],[162,3,162,4],[162,6,162,7],[163,3,163,4],[163,6,163,7],[164,3,164,4],[164,6,164,7],[165,3,165,4],[165,6,165,7],[166,3,166,4],[166,6,166,7],[167,3,167,4],[167,6,167,7],[168,3,168,4],[168,6,168,7],[169,3,169,4],[169,6,169,7],[170,3,170,4],[170,6,170,7],[171,3,171,4],[171,6,171,7],[172,3,172,4],[172,6,172,7],[173,3,173,4],[173,6,173,7],[174,3,174,4],[174,6,174,7],[175,0,175,8],[176,0,176,9],[177,0,177,3],[177,4,177,6],[177,7,177,9],[178,0,179,0],[178,1,179,1],[178,2,179,2],[178,3,179,4],[178,5,179,5],[178,6,179,7],[178,8,178,9],[180,3,180,4],[180,6,180,7],[181,3,181,4],[181,6,181,7],[182,3,182,4],[182,6,182,7],[183,3,183,4],[183,6,183,7],[184,3,184,4],[184,6,184,7],[185,3,185,4],[185,6,185,7],[186,3,186,4],[186,6,186,7],[187,3,187,4],[187,6,187,7],[188,3,188,4],[188,6,188,7],[189,3,189,4],[189,6,189,7],[190,3,190,4],[190,6,190,7],[191,3,191,4],[191,6,191,7],[192,3,192,4],[192,6,192,7],[193,0,193,8],[194,0,194,9],[195,0,195,3],[195,4,195,6],[195,7,195,9],[196,0,197,0],[196,1,197,1],[196,2,197,2],[196,3,197,4],[196,5,197,5],[196,6,197,7],[196,8,196,9],[198,3,198,4],[198,6,198,7],[199,3,199,4],[199,6,199,7],[200,3,200,4],[200,6,200,7],[201,3,201,4],[201,6,201,7],[202,3,202,4],[202,6,202,7],[203,3,203,4],[203,6,203,7],[204,3,204,4],[204,6,204,7],[205,3,205,4],[205,6,205,7],[206,3,206,4],[206,6,206,7],[207,3,207,4],[207,6,207,7],[208,3,208,4],[208,6,208,7],[209,3,209,4],[209,6,209,7],[210,0,210,8],[211,0,211,9],[212,0,212,3],[212,4,212,6],[212,7,212,9],[213,0,214,0],[213,1,214,1],[213,2,214,2],[213,3,214,4],[213,5,214,5],[213,6,214,7],[213,8,213,9],[215,3,215,4],[215,6,215,7],[216,3,216,4],[216,6,216,7],[217,3,217,4],[217,6,217,7],[218,3,218,4],[218,6,218,7],[219,3,219,4],[219,6,219,7],[220,3,220,4],[220,6,220,7],[221,3,221,4],[221,6,221,7],[222,3,222,4],[222,6,222,7],[223,3,223,4],[223,6,223,7],[224,3,224,4],[224,6,224,7],[225,3,225,4],[225,6,225,7],[226,3,226,4],[226,6,226,7],[227,3,227,4],[227,6,227,7],[228,3,228,4],[228,6,228,7],[229,0,229,8],[230,0,230,9],[231,0,231,3],[231,4,231,6],[231,7,231,9],[232,0,233,0],[232,1,233,1],[232,2,233,2],[232,3,233,4],[232,5,233,5],[232,6,233,7],[232,8,232,9],[234,3,234,4],[234,6,234,7],[235,3,235,4],[235,6,235,7],[236,3,236,4],[236,6,236,7],[237,3,237,4],[237,6,237,7],[238,3,238,4],[238,6,238,7],[239,3,239,4],[239,6,239,7],[240,3,240,4],[240,6,240,7],[241,3,241,4],[241,6,241,7],[242,3,242,4],[242,6,242,7],[243,3,243,4],[243,6,243,7],[244,3,244,4],[244,6,244,7],[245,3,245,4],[245,6,245,7],[246,3,246,4],[246,6,246,7],[247,3,247,4],[247,6,247,7],[248,3,248,4],[248,6,248,7],[249,3,249,4],[249,6,249,7],[250,3,250,4],[250,6,250,7],[251,3,251,4],[251,6,251,7],[252,0,252,8],[253,0,253,8]],"flags":["formulas_cached_only"]}
["劳务报价明细表"]
["工程名称：建筑与装饰工程",{"$nulls":6},"第 1 页  共 17 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量\n单位","工程量",null,"金额（元）"]
[{"$nulls":8},"劳务单价","合价"]
[null,null,"一层东大厅"]
[1,"01B001","拆除吊顶","1.拆除室内吊顶及\n龙骨",null,"m2",72.49]
[2,"01B002","拆除墙面装饰","1.拆除墙面装饰墙\n面板及龙骨",null,"m2",26.3]
[3,"01B003","拆除书柜","1.拆除靠墙书柜",null,"m2",7.76]
[4,"01B005","拆除服务台","1.拆除服务台",null,"m2",2.34]
[5,"01B007","拆除涂料","1.铲除墙面乳胶漆",null,"m2",55.79]
[6,"01B008","拆除踢脚线","1.拆除踢脚线",null,"m",22.55]
[7,"011205001001","墙、柱面装饰板","1.龙骨材料种类、\n规格、中距:75轻钢\n龙骨（共二层）\n2. 隔离层材料种类\n、规格:50mm吸音棉\n（容重80kg/m³ )   (\n共二层）\n3. 隔离层材料种类\n、规格:3mm隔音毡\n（共三层）\n4.基层材料种类、\n规格:12mm石膏板基\n层（共四层）\n5.面层材料品种、\n规格:12mm石膏板面\n层（共二层）",null,"m2",31.9]
[8,"011404001001","墙面喷刷涂料","1. 喷刷涂料部位 : 内\n墙面\n2.腻子种类:成品腻\n子\n3.刮腻子遍数:2遍\n4.涂料品种、喷刷\n遍数:防火型合成树\n脂乳液两遍\n5.位置:房间内的石\n膏板墙面上",null,"m2",24.65]
["本页小计"]
["劳务报价明细表"]
["工程名称：建筑与装饰工程",{"$nulls":6},"第 2 页  共 17 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量\n单位","工程量",null,"金额（元）"]
[{"$nulls":8},"劳务单价","合价"]
[9,"011403001001","抹灰面油漆","1.腻子种类:成品腻\n子\n2.刮腻子遍数:2遍\n3. 防护材料种类:封\n底漆一道\n4.油漆品种、刷漆\n遍数:乳胶漆两遍\n5.位置：  原墙面刷\n乳胶漆",null,"m2",98.6]
[10,"011404001002","墙面喷刷涂料","1. 喷刷涂料部位 : 内\n墙面\n2.涂料品种、喷刷\n遍数:无机涂料两遍\n3.位置:走廊的石膏\n板墙面上",null,"m2",26.22]
[11,"011105006001","金属踢脚线","1.面层材料品种、\n规格:不锈钢踢脚，\n配套胶粘接\n2.踢脚线高度100mm",null,"m",17.74]
[12,"011105003001","块料踢脚线","1.结合层厚度、材\n料种类及强度等级 :\n10厚1:2水泥砂浆粘\n结层 ，素水泥浆一道\n甩毛（内掺建筑胶）\n2.面层材料品种、\n规格:10厚铺地砖踢\n脚 ，稀水泥浆擦缝，\n缝宽8\n3.踢脚线高度100mm",null,"m",37.84]
[13,"011302001001","平面吊顶天棚","1.龙骨材料种类、\n规格、中距:轻钢龙\n骨\n2.面板材料品种、\n规格:600*600矿棉\n板吊顶",null,"m2",71.54]
["本页小计"]
["劳务报价明细表"]
["工程名称：建筑与装饰工程",{"$nulls":6},"第 3 页  共 17 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量\n单位","工程量",null,"金额（元）"]
[{"$nulls":8},"劳务单价","合价"]
[14,"010801002001","木质门带套","1. 门洞口尺寸:M102\n2\n2. 门类型:成品室内\n门\n3.开启方式:平开\n4.含门锁及配套五\n金件",null,"m2",2.2]
[15,"010810002007","窗帘盒","1. 窗帘盒材质、规\n格:木龙骨、9mm胶\n合板基层、12mm石\n膏板",null,"m",6.4]
[null,null,"一层会议室改造"]
[16,"01B009","拆除砌体墙","1.掏砌门洞 ，墙体\n厚度200mm",null,"m2",2.2]
[17,"01B010","拆除涂料","1.铲除墙面乳胶漆",null,"m2",57.84]
[18,"01B011","拆除踢脚线","1.拆除踢脚线",null,"m",24.5]
[19,"010801002002","木质门带套","1. 门洞口尺寸:M102\n2\n2. 门类型:成品室内\n门\n3.开启方式:平开\n4.含门锁及配套五\n金件",null,"m2",2.2]
[20,"010402001001","砌块墙","1.砌块品种、规格\n、强度等级:蒸压加\n气混凝土砌块 ，M5\n水泥砂浆砌筑\n2.墙体类型 : 内墙\n3.墙体厚度 :200mm",null,"m3",3.34]
[21,"011201001001","墙、柱面一般抹灰","1.5厚1:2水泥砂浆\n2. 15厚1:3水泥砂浆\n打底扫毛\n3.素水泥浆一道甩\n毛(内掺建筑胶)\n4.位置：新建隔墙\n抹灰",null,"m2",33.35]
["本页小计"]
["劳务报价明细表"]
["工程名称：建筑与装饰工程",{"$nulls":6},"第 4 页  共 17 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量\n单位","工程量",null,"金额（元）"]
[{"$nulls":8},"劳务单价","合价"]
[22,"011404001003","墙面喷刷涂料","1. 喷刷涂料部位 : 内\n墙面\n2.腻子种类:成品腻\n子\n3.刮腻子遍数:2遍\n4.涂料品种、喷刷\n遍数:防火型合成树\n脂乳液两遍\n5.位置:新建隔墙刷\n乳胶漆",null,"m2",32.2]
[23,"011403001002","抹灰面油漆","1.腻子种类:成品腻\n子\n2.刮腻子遍数:2遍\n3. 防护材料种类:封\n底漆一道\n4.油漆品种、刷漆\n遍数:乳胶漆两遍\n5.位置：  原墙面刷\n乳胶漆",null,"m2",57.48]
[24,"011105003002","块料踢脚线","1.结合层厚度、材\n料种类及强度等级 :\n10厚1:2水泥砂浆粘\n结层 ，素水泥浆一道\n甩毛（内掺建筑胶）\n2.面层材料品种、\n规格:10厚铺地砖踢\n脚 ，稀水泥浆擦缝，\n缝宽8\n3.踢脚线高度100mm",null,"m",34.6]
[25,"010810002006","窗帘盒","1. 窗帘盒材质、规\n格:木龙骨、9mm胶\n合板基层、12mm石\n膏板",null,"m",7.5]
[null,null,"二层大厅改造"]
[26,"01B015","拆除吊顶","1.拆除室内吊顶及\n龙骨",null,"m2",75.67]
[27,"01B016","拆除金属门窗","1.拆除外墙固定窗户",null,"m2",37.02]
["本页小计"]
["劳务报价明细表"]
["工程名称：建筑与装饰工程",{"$nulls":6},"第 5 页  共 17 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量\n单位","工程量",null,"金额（元）"]
[{"$nulls":8},"劳务单价","合价"]
[28,"010402001003","砌块墙","1.砌块品种、规格\n、强度等级:蒸压加\n气混凝土砌块 ，M5\n水泥砂浆砌筑\n2.墙体类型:外墙\n3.墙体厚度 :300mm",null,"m3",7.75]
[29,"011205001002","墙、柱面装饰板","1.龙骨材料种类、\n规格、中距:75轻钢\n龙骨（共二层）\n2. 隔离层材料种类\n、规格:50mm吸音棉\n（容重80kg/m³ )   (\n共二层）\n3. 隔离层材料种类\n、规格:3mm隔音毡\n（共三层）\n4.基层材料种类、\n规格:12mm石膏板基\n层（共四层）\n5.面层材料品种、\n规格:12mm石膏板面\n层（共二层）",null,"m2",80.01]
[30,"010807001001","金属(塑钢)窗","1. 窗洞口尺寸:C212\n0 、MLC2129中的窗\n2.开启方式 : 内平开\n3.框、扇材质及规\n格:70系列隔热铝合\n金窗\n4.玻璃品种、厚度 :\n5+12A+5Low-E+12A\n+5Low-E",null,"m2",15.76]
[31,"010802001001","金属(塑钢)门","1. 门洞口尺寸:MLC2\n129中的门800*2200\n2.开启方式:平开\n3.框、扇材质:70系\n列隔热铝合金门\n4.玻璃品种、厚度 :\n5+12A+5Low-E+12A\n+5Low-E",null,"m2",1.76]
[32,"010809001001","窗台板","1. 窗台板材质、规\n格:大理石材质",null,"m2",1.52]
["本页小计"]
["劳务报价明细表"]
["工程名称：建筑与装饰工程",{"$nulls":6},"第 6 页  共 17 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量\n单位","工程量",null,"金额（元）"]
[{"$nulls":8},"劳务单价","合价"]
[33,"011201001003","墙、柱面一般抹灰","1.5厚1:2水泥砂浆\n2. 15厚1:3水泥砂浆\n打底扫毛\n3.素水泥浆一道甩\n毛(内掺建筑胶)\n4.位置：新建隔墙\n抹灰",null,"m2",17.82]
[34,"011404001005","墙面喷刷涂料","1. 喷刷涂料部位 : 内\n墙面\n2.腻子种类:成品腻\n子\n3.刮腻子遍数:2遍\n4.涂料品种、喷刷\n遍数:防火型合成树\n脂乳液两遍\n5.位置:新建隔墙刷\n乳胶漆",null,"m2",16.55]
[35,"011404001006","墙面喷刷涂料","1. 喷刷涂料部位 : 内\n墙面\n2.腻子种类:成品腻\n子\n3.刮腻子遍数:2遍\n4.涂料品种、喷刷\n遍数:防火型合成树\n脂乳液两遍\n5.位置:房间内的石\n膏板墙面上",null,"m2",100.45]
[36,"011404001007","墙面喷刷涂料","1. 喷刷涂料部位 : 内\n墙面\n2.涂料品种、喷刷\n遍数:无机涂料两遍\n3.位置:走廊的石膏\n板墙面上",null,"m2",22.85]
["本页小计"]
["劳务报价明细表"]
["工程名称：建筑与装饰工程",{"$nulls":6},"第 7 页  共 17 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量\n单位","工程量",null,"金额（元）"]
[{"$nulls":8},"劳务单价","合价"]
[37,"011105003004","块料踢脚线","1.结合层厚度、材\n料种类及强度等级 :\n10厚1:2水泥砂浆粘\n结层 ，素水泥浆一道\n甩毛（内掺建筑胶）\n2.面层材料品种、\n规格:10厚铺地砖踢\n脚 ，稀水泥浆擦缝，\n缝宽8\n3.踢脚线高度100mm",null,"m",12.1]
[38,"011105006002","金属踢脚线","1.面层材料品种、\n规格:不锈钢踢脚，\n配套胶粘接\n2.踢脚线高度100mm",null,"m",44.78]
[39,"011302001002","平面吊顶天棚","1.龙骨材料种类、\n规格、中距:轻钢龙\n骨\n2.面板材料品种、\n规格:600*600矿棉\n板吊顶",null,"m2",68.2]
[40,"010801002003","木质门带套","1. 门洞口尺寸:M102\n4\n2. 门类型:成品室内\n门\n3.开启方式:平开\n4.含门锁及配套五\n金件",null,"m2",9.6]
[41,"010810002005","窗帘盒","1. 窗帘盒材质、规\n格:木龙骨、9mm胶\n合板基层、12mm石\n膏板",null,"m",12.9]
[42,"010810001004","窗帘","1. 窗帘材质:百叶窗\n帘",null,"m2",15.2]
[43,"01B017","开启扇外开","1.开启扇外开\n2.尺寸1.2*0.6m",null,"个",2]
["本页小计"]
["劳务报价明细表"]
["工程名称：建筑与装饰工程",{"$nulls":6},"第 8 页  共 17 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量\n单位","工程量",null,"金额（元）"]
[{"$nulls":8},"劳务单价","合价"]
[44,"011201001004","墙、柱面一般抹灰","1.基层类型、部位 :\n外墙\n2.各层厚度、材料\n种类及强度等级 : 15\nmm厚1:3水泥砂浆找\n平",null,"m2",25.82]
[45,"011001003001","保温隔热墙面","1. 100厚挤塑板保温\n板,配套胶粘贴剂粘\n贴,铺锚栓固定\n2. 15厚干粉类聚合\n物水泥防水砂浆, 中\n间压入一层耐碱玻璃\n纤维网布",null,"m2",25.82]
[46,"011404001008","墙面喷刷涂料","1.刮柔性耐水腻子\n2. 喷或滚刷底涂料\n3. 喷或滚刷面层涂",null,"m2",25.82]
[47,"011205001003","墙、柱面装饰板","1. 隔离层材料种类\n、规格:3mm隔音毡\n（共二层）\n2.基层材料种类、\n规格:12mm石膏板基\n层\n3.面层材料品种、\n规格:12mm石膏板面\n层\n4.位置：石膏板包\n柱脚",null,"m2",6.94]
[null,null,"三、四、五、六\n开水间改造"]
[48,"01B012","拆除砌体墙","1.掏砌门洞 ，墙体\n厚度200mm",null,"m2",7.2]
[49,"01B013","拆除涂料","1.铲除墙面乳胶漆",null,"m2",112.16]
[50,"01B014","拆除踢脚线","1.拆除踢脚线",null,"m",44]
[51,"010402001002","砌块墙","1.砌块品种、规格\n、强度等级:蒸压加\n气混凝土砌块 ，M5\n水泥砂浆砌筑\n2.墙体类型 : 内墙\n3.墙体厚度 : 100mm",null,"m3",1.96]
["本页小计"]
["劳务报价明细表"]
["工程名称：建筑与装饰工程",{"$nulls":6},"第 9 页  共 17 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量\n单位","工程量",null,"金额（元）"]
[{"$nulls":8},"劳务单价","合价"]
[52,"011108003001","块料零星项目","1.面层材料品种、\n规格:陶瓷地砖",null,"m2",3.6]
[53,"011201001002","墙、柱面一般抹灰","1.5厚1:2水泥砂浆\n2. 15厚1:3水泥砂浆\n打底扫毛\n3.素水泥浆一道甩\n毛(内掺建筑胶)\n4.位置：新建隔墙\n抹灰",null,"m2",39.2]
[54,"011404001004","墙面喷刷涂料","1. 喷刷涂料部位 : 内\n墙面\n2.腻子种类:成品腻\n子\n3.刮腻子遍数:2遍\n4.涂料品种、喷刷\n遍数:防火型合成树\n脂乳液两遍\n5.位置:新建隔墙刷\n乳胶漆",null,"m2",37.8]
[55,"011403001003","抹灰面油漆","1.腻子种类:成品腻\n子\n2.刮腻子遍数:2遍\n3. 防护材料种类:封\n底漆一道\n4.油漆品种、刷漆\n遍数:乳胶漆两遍\n5.位置：  原墙面刷\n乳胶漆",null,"m2",108.92]
[56,"011105003003","块料踢脚线","1.结合层厚度、材\n料种类及强度等级 :\n10厚1:2水泥砂浆粘\n结层 ，素水泥浆一道\n甩毛（内掺建筑胶）\n2.面层材料品种、\n规格:10厚铺地砖踢\n脚 ，稀水泥浆擦缝，\n缝宽8\n3.踢脚线高度100mm",null,"m",39.6]
[null,null,"八层大厅改造"]
["本页小计"]
["劳务报价明细表"]
["工程名称：建筑与装饰工程",{"$nulls":6},"第 10 页  共 17 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量\n单位","工程量",null,"金额（元）"]
[{"$nulls":8},"劳务单价","合价"]
[57,"01B018","拆除地面","1.拆除地面木地板",null,"m2",35.46]
[58,"01B019","拆除吊顶","1.拆除室内吊顶及\n龙骨",null,"m2",147.07]
[59,"01B020","拆除墙面装饰","1.拆除附墙矮柜、\n展柜、背景墙、石膏\n板隔墙、广告、书架\n、装饰构件等",null,"m2",56.71]
[60,"01B021","拆除门","1.拆除子母套装门",null,"m2",2.52]
[61,"01B022","拆除涂料","1.铲除墙面乳胶漆",null,"m2",97.47]
[62,"01B023","拆除踢脚线","1.拆除踢脚线",null,"m",46.13]
[63,"011102003001","块料楼地面","1.结合层厚度、材\n料种类及强度等级 :\n1:3水泥砂浆20mm厚\n2.面层材料品种、\n规格:陶瓷地砖  800\n*800mm",null,"m2",35.46]
[64,"011105006003","金属踢脚线","1.面层材料品种、\n规格:不锈钢踢脚，\n配套胶粘接\n2.踢脚线高度100mm",null,"m",124.87]
[65,"011205001004","墙、柱面装饰板","1.龙骨材料种类、\n规格、中距:75轻钢\n龙骨（共二层）\n2. 隔离层材料种类\n、规格:50mm吸音棉\n（容重80kg/m³ )   (\n共二层）\n3. 隔离层材料种类\n、规格:3mm隔音毡\n（共三层）\n4.基层材料种类、\n规格:12mm石膏板基\n层（共四层）\n5.面层材料品种、\n规格:12mm石膏板面\n层（共二层）",null,"m2",122.22]
["本页小计"]
["劳务报价明细表"]
["工程名称：建筑与装饰工程",{"$nulls":6},"第 11 页  共 17 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量\n单位","工程量",null,"金额（元）"]
[{"$nulls":8},"劳务单价","合价"]
[66,"011404001009","墙面喷刷涂料","1. 喷刷涂料部位 : 内\n墙面\n2.腻子种类:成品腻\n子\n3.刮腻子遍数:2遍\n4.涂料品种、喷刷\n遍数:防火型合成树\n脂乳液两遍\n5.位置:房间内的石\n膏板墙面上",null,"m2",167.43]
[67,"011403001004","抹灰面油漆","1.腻子种类:成品腻\n子\n2.刮腻子遍数:2遍\n3. 防护材料种类:封\n底漆一道\n4.油漆品种、刷漆\n遍数:乳胶漆两遍\n5.位置：  原墙面刷\n乳胶漆",null,"m2",131.65]
[68,"011404001010","墙面喷刷涂料","1. 喷刷涂料部位 : 内\n墙面\n2.涂料品种、喷刷\n遍数:无机涂料两遍\n3.位置:走廊的石膏\n板墙面上",null,"m2",60.5]
[69,"011302001003","平面吊顶天棚","1.龙骨材料种类、\n规格、中距:轻钢龙\n骨\n2.面板材料品种、\n规格:600*600矿棉\n板吊顶",null,"m2",138.05]
[70,"010801002004","木质门带套","1. 门洞口尺寸:M102\n4\n2. 门类型:成品室内\n门\n3.开启方式:平开\n4.含门锁及配套五\n金件",null,"m2",14.4]
["本页小计"]
["劳务报价明细表"]
["工程名称：建筑与装饰工程",{"$nulls":6},"第 12 页  共 17 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量\n单位","工程量",null,"金额（元）"]
[{"$nulls":8},"劳务单价","合价"]
[71,"010810002004","窗帘盒","1. 窗帘盒材质、规\n格:木龙骨、9mm胶\n合板基层、12mm石\n膏板",null,"m",19.19]
[72,"010810001003","窗帘","1. 窗帘材质:百叶窗\n帘",null,"m2",27.8]
[73,"011205001005","墙、柱面装饰板","1. 隔离层材料种类\n、规格:3mm隔音毡\n（共二层）\n2.基层材料种类、\n规格:12mm石膏板基\n层\n3.面层材料品种、\n规格:12mm石膏板面\n层\n4.位置：石膏板包\n柱脚",null,"m2",16.4]
[null,null,"建筑垃圾外运"]
[74,"010103002006","余方弃置","1.建筑垃圾装载机\n装车外运16km",null,"m3",35.65]
{"$rows_empty":18}
["本页小计"]
["劳务报价明细表"]
["工程名称：电气设备安装工程",{"$nulls":6},"第 13页  共 17 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量\n单位","工程量",null,"金额（元）"]
[{"$nulls":8},"劳务单价","合价"]
[null,null,"一层"]
[1,"03B001","筒灯拆除","1.名称:筒灯拆除",null,"套",31]
[2,"030413001001","普通灯具","1.名称：方形灯\n2.规格：600*600",null,"套",6]
[3,"030413014001","插座","1.名称：普通五孔\n插座\n2.规格：  10A\n3.安装方式：  暗装",null,"套",4]
[4,"030413014004","插座","1.名称：  空调插座\n2.规格：  16A\n3.安装方式：  暗装",null,"套",1]
[5,"030413013001","照明开关、按钮","1.名称：三联开关\n2.规格：  10V\n3.安装方式：  暗装",null,"套",1]
[6,"030502010001","信息、网络插座","1.名称：双口信息\n插座（外网）",null,"个",1]
[7,"030502010004","信息、网络插座","1.名称：  四口信息\n插座（内网）",null,"个",1]
[8,"030412006001","接线盒","1.名称：接线盒\n2.材质：塑料\n3.安装方式：  暗装",null,"个",14]
[9,"030502003001","双绞线缆","1.名称：超六类网线",null,"m",96.46]
[10,"030502005001","光缆","1.名称：单模光纤",null,"m",171.4]
[11,"030412001004","配管","1.名称：配管\n2.规格、材质：JDG\n25\n3.配置形式：    砖、\n混凝土结构暗配",null,"m",17.12]
[12,"030412001001","配管","1.名称：配管\n2.规格、材质：PVC\n20\n3.配置形式：    砖、\n混凝土结构暗配",null,"m",64.5]
["本页小计"]
["劳务报价明细表"]
["工程名称：电气设备安装工程",{"$nulls":6},"第 14 页  共 17 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量\n单位","工程量",null,"金额（元）"]
[{"$nulls":8},"劳务单价","合价"]
[13,"030412004001","配线","1.名称：配线\n2.规格：BV4\n3.敷设方式：  管内\n穿线",null,"m",351.65]
[14,"030412004002","配线","1.名称：配线\n2.规格：BV2.5\n3.敷设方式：  管内\n穿线",null,"m",125.7]
[15,"030412004003","配线","1.名称：配线\n2.规格：NH-RVS-2*\n1.5\n3.敷设方式：  管内\n穿线",null,"m",20]
[16,"03B005","拆除球型摄像机","1.名称:拆除球型摄像机",null,"台",3]
[17,"030506010001","监控摄像设备","1.名称：安装原有\n半球摄像机",null,"台",3]
[18,"030506010002","监控摄像设备","1.名称：新增半球\n摄像机",null,"台",1]
[null,null,"二层"]
[19,"03B006","筒灯拆除","1.名称:筒灯拆除",null,"套",22]
[20,"030413001002","普通灯具","1.名称：方形灯\n2.规格：600*600",null,"套",8]
[21,"030413014002","插座","1.名称：普通五孔\n插座\n2.规格：  10A\n3.安装方式：  暗装",null,"套",9]
[22,"030413014005","插座","1.名称：  空调插座\n2.规格：  16A\n3.安装方式：  暗装",null,"套",4]
[23,"030413013002","照明开关、按钮","1.名称：三联开关\n2.规格：  10V\n3.安装方式：  暗装",null,"套",4]
[24,"030502010005","信息、网络插座","1.名称：双口信息\n插座（外网）",null,"个",4]
["本页小计"]
["劳务报价明细表"]
["工程名称：电气设备安装工程",{"$nulls":6},"第 15 页  共 17 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量\n单位","工程量",null,"金额（元）"]
[{"$nulls":8},"劳务单价","合价"]
[25,"030502010006","信息、网络插座","1.名称：  四口信息\n插座（内网）",null,"个",4]
[26,"030412006002","接线盒","1.名称：接线盒\n2.材质：塑料\n3.安装方式：  暗装",null,"个",33]
[27,"030502003002","双绞线缆","1.名称：超六类网线",null,"m",159.58]
[28,"030502005002","光缆","1.名称：单模光纤",null,"m",290.36]
[29,"030412001005","配管","1.名称：配管\n2.规格、材质：JDG\n25\n3.配置形式：    砖、\n混凝土结构暗配",null,"m",54.4]
[30,"030412001002","配管","1.名称：配管\n2.规格、材质：PVC\n20\n3.配置形式：    砖、\n混凝土结构暗配",null,"m",160.01]
[31,"030412004004","配线","1.名称：配线\n2.规格：BV4\n3.敷设方式：  管内\n穿线",null,"m",891.38]
[32,"030412004005","配线","1.名称：配线\n2.规格：BV2.5\n3.敷设方式：  管内\n穿线",null,"m",144.2]
[33,"03B009","拆除暖气管道","1.名称:拆除暖气管\n道\n2.规格:DN25\n3.材质:镀锌钢管",null,"m",2]
[34,"03B010","拆除散热器","1.名称:拆除散热器\n2.规格:25片",null,"组",2]
[35,"030701003004","空调器","1.名称：挂墙式空\n调\n2.安装方式：挂墙",null,"台",2]
[36,"031004001001","铸铁散热器","1.名称：安装原有\n铸铁散热器\n2.规格：25片",null,"组",2]
["本页小计"]
["劳务报价明细表"]
["工程名称：电气设备安装工程",{"$nulls":6},"第 16 页  共 17页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量\n单位","工程量",null,"金额（元）"]
[{"$nulls":8},"劳务单价","合价"]
[37,"031004001002","铸铁散热器","1.名称：铸铁散热\n器\n2.规格：25片\n3.安装方式：壁挂",null,"组",4]
[38,"031001002001","镀锌钢管","1.安装部位：室内\n2.介质：采暖\n3.材质：镀锌钢管\n4.规格：DN25\n5.连接方式：螺纹\n连接",null,"m",20]
[39,"031002001001","金属阀门","1.名称：截止阀\n2.规格：DN25\n3.连接方式：螺纹\n连接",null,"个",8]
[null,null,"八层"]
[40,"03B012","筒灯拆除","1.名称:筒灯拆除",null,"套",83]
[41,"03B013","筒灯拆除","1.名称:射灯拆除",null,"套",10]
[42,"030413001003","普通灯具","1.名称：方形灯\n2.规格：600*600",null,"套",16]
[43,"030413014003","插座","1.名称：普通五孔\n插座\n2.规格：  10A\n3.安装方式：  暗装",null,"套",12]
[44,"030413014006","插座","1.名称：  空调插座\n2.规格：  16A\n3.安装方式：  暗装",null,"套",5]
[45,"030413013003","照明开关、按钮","1.名称：三联开关\n2.规格：  10V\n3.安装方式：  暗装",null,"套",6]
[46,"030502010007","信息、网络插座","1.名称：双口信息\n插座（外网）",null,"个",5]
[47,"030502010008","信息、网络插座","1.名称：  四口信息\n插座（内网）",null,"个",5]
[48,"030412006003","接线盒","1.名称：接线盒\n2.材质：塑料\n3.安装方式：  暗装",null,"个",49]
[49,"030502003003","双绞线缆","1.名称：超六类网线",null,"m",246.6]
["本页小计"]
["劳务报价明细表"]
["工程名称：电气设备安装工程",{"$nulls":6},"第 17页  共 17页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量\n单位","工程量",null,"金额（元）"]
[{"$nulls":8},"劳务单价","合价"]
[50,"030502005003","光缆","1.名称：单模光纤",null,"m",890.72]
[51,"030412001006","配管","1.名称：配管\n2.规格、材质：JDG\n25\n3.配置形式：    砖、\n混凝土结构暗配",null,"m",144.6]
[52,"030412001003","配管","1.名称：配管\n2.规格、材质：PVC\n20\n3.配置形式：    砖、\n混凝土结构暗配",null,"m",287.68]
[53,"030412004007","配线","1.名称：配线\n2.规格：BV4\n3.敷设方式：  管内\n穿线",null,"m",986.1]
[54,"030412004008","配线","1.名称：配线\n2.规格：BV2.5\n3.敷设方式：  管内\n穿线",null,"m",268.54]
[55,"03B014","拆除风机","1.名称 : 吊顶式室内\n机",null,"台",1]
[56,"030701003005","空调器","1.名称：安装原有\n空调室内机",null,"台",1]
[57,"030701003007","空调器","1.名称：挂墙式空\n调\n2.安装方式：挂墙",null,"台",4]
{"$rows_empty":10}
["本页小计"]
["合    计"]